# RDS95

(eRT)(RDS2)

RDS95 is a light software RDS encoder for linux

RDS95 also embeds Lua to implement some things

RDS95 follows the IEC 62106 standard (available at the RDS Forum website)

## Diffrences between IEC 62106 and EN 50067

The newer standard which is the IEC one, removes these features:

- MS
- PIN
- LIC
- DI (partially, only dynamic pty is left)
- EWS (now ODA)
- IH (now ODA)
- RP
- TDC (now ODA)

## Unique features

RDS95 is the only (as far as i can tell) encoder to transmit the 9-bit AF codes

## Lua engine

Yet another unique feature, the Lua engine allows you to control the encoder, almost entirely.

Every RDS2 subcarrier is in full control of Lua (except tunneling - core fills in PTY and the rest)
